[:SENSe]:WCDMa:CHANnel:DESPread:DLINk:TRACe[:SELection] | command/query

Gets or sets which data is presented in the Despread1 and Despread2 traces.

Command Syntax: | [:SENSe]:WCDMa:CHANnel:DESPread:DLINk:TRACe[:SELection] <value>
<value> | ::= | "Normal" | "HSTRBlock" | "HSTRBlock1PerAntenna" | "HSTRBlock2PerAntenna"
Query Syntax: | [:SENSe]:WCDMa:CHANnel:DESPread:DLINk:TRACe[:SELection]?
Returns | ::= | "Normal" | "HSTRBlock" | "HSTRBlock1PerAntenna" | "HSTRBlock2PerAntenna"
Remarks: | <none>
Example: |
    :WCDM:CHAN:DESP:DLIN:TRAC "Normal"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.DespreadTraceSelection Agilent.SA.Vsa.Wcdma.DespreadTraceSelection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |