[:SENSe]:TDSCdma:ADVanced:SLOT:THReshold | command/query

Gets or sets the threshold for detecting an active time slot relative to the power of the highest amplitude time slot (in dBc).

Command Syntax: | [:SENSe]:TDSCdma:ADVanced:SLOT:THReshold <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:TDSCdma:ADVanced:SLOT:THReshold?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Tdscdma.Interfaces.MeasurementExtension.ActiveSlotThreshold

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |