[:SENSe]:TDSCdma:CHANnel:MOD:DETect | command/query

Gets or sets a value indicating whether the modulation type is automatically determined or not.

Command Syntax: | [:SENSe]:TDSCdma:CHANnel:MOD:DETect <value>
<value> | ::= | "Automatic" | "Manual"
Query Syntax: | [:SENSe]:TDSCdma:CHANnel:MOD:DETect?
Returns | ::= | "Automatic" | "Manual"
Remarks: | <none>
Example: |
    :TDSC:CHAN:MOD:DET "Automatic"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Tdscdma.Interfaces.MeasurementExtension.ModulationDetect Agilent.SA.Vsa.Tdscdma.ModulationDetectType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |