[:SENSe]:W11B[:FORMat]:MODulation | command/query

Gets or sets the modulation format of the data part of the burst.

Command Syntax: | [:SENSe]:W11B[:FORMat]:MODulation <value>
<value> | ::= | "Barker1" | "Barker2" | "Cck5" | "Cck11" | "Pbcc5" | "Pbcc11" | "Pbcc22" | "Pbcc33"
Query Syntax: | [:SENSe]:W11B[:FORMat]:MODulation?
Returns | ::= | "Barker1" | "Barker2" | "Cck5" | "Cck11" | "Pbcc5" | "Pbcc11" | "Pbcc22" | "Pbcc33"
Remarks: | <none>
Example: |
    :W11B:MOD "Barker1"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211BG.Interfaces.MeasurementExtension.DataModulation Agilent.SA.Vsa.Wlan80211BG.DataModulation

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |