[:SENSe]:W11B:ADVanced:CRATe | command/query

Gets or sets the chip rate of the measured signal

Command Syntax: | [:SENSe]:W11B:ADVanced:CRATe <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:W11B:ADVanced:CRATe?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211BG.Interfaces.MeasurementExtension.ChipRate

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |