[:SENSe]:W11N[:FORMat]:CHANnel:ENABle | command/query

Gets or sets which of the available input channels will be analyzed.

Command Syntax: | [:SENSe]:W11N[:FORMat]:CHANnel:ENABle <enabledChs>
<enabledChs> | ::= | Comma separated values of 0 | 1
Query Syntax: | [:SENSe]:W11N[:FORMat]:CHANnel:ENABle?
Returns | ::= | Comma separated values of Integer number
Remarks: | <none>
Example: |
    :W11N:CHAN:ENAB 0,0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211N.Interfaces.MeasurementExtension.InputChannels

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |