[:SENSe]:LTE:PROFile:SSCH:ENABle | command/query

Gets or sets a value indicating whether S-SS is enabled in trace displays and included in overall EVM calculation.

Command Syntax: | [:SENSe]:LTE:PROFile:SSCH:ENABle <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:SSCH:ENABle?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:PROF:SSCH:ENAB 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.IsSschEnabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |