[:SENSe]:W11N[:FORMat]:SMAPping | command/query

Gets or sets the type of spatial mapping matrix used by the transmitter.

Command Syntax: | [:SENSe]:W11N[:FORMat]:SMAPping <value>
<value> | ::= | "DirectMap" | "Fourier" | "DirectMap2" | "Fourier2" | "Automatic"
Query Syntax: | [:SENSe]:W11N[:FORMat]:SMAPping?
Returns | ::= | "DirectMap" | "Fourier" | "DirectMap2" | "Fourier2" | "Automatic"
Remarks: | <none>
Example: |
    :W11N:SMAP "DirectMap"
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211N.Interfaces.MeasurementExtension.SpatialMappingMatrixSelection Agilent.SA.Vsa.Wlan80211N.SpatialMappingMatrixSelection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |