[:SENSe]:W16E:TIME:REGion | command/query

Gets or sets a value indicating whether to use the measurement offset and interval parameters or whether the analysis should choose the measurement region automatically.

Command Syntax: | [:SENSe]:W16E:TIME:REGion <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:W16E:TIME:REGion?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :W16E:TIME:REG 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.IsMeasurementRegionEnabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |