:INPut:ANALog:IMPedance:LIST | command/query

Gets or sets the impedance for the input connection.

Command Syntax: | :INPut:ANALog:IMPedance:LIST <impedanceBaseUnits>
<impedanceBaseUnits> | ::= | Comma separated values of Real number
Query Syntax: | :INPut:ANALog:IMPedance:LIST?
Returns | ::= | Comma separated values of Real number
Remarks: | <none>
Example: |
    :INP:ANAL:IMP:LIST 50.0,50.0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.AnalogChannel.Impedance

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |