[:SENSe]:LTE[:FORMat]:PRESet | command

Preset all measurement attributes to their defaults for the indicated bandwidth

Command Syntax: | [:SENSe]:LTE[:FORMat]:PRESet <standard>
<standard> | ::= | "BW1P4Mhz6RB" | "BW3Mhz15RB" | "BW5Mhz25RB" | "BW10Mhz50RB" | "BW15Mhz75RB" | "BW20Mhz100RB"
Remarks: | <none>
Example: |
    :LTE:PRES "BW1P4Mhz6RB"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.Preset Agilent.SA.Vsa.Lte.StandardsType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |