[:SENSe]:WCDMa[:FORMat]:SCRamble:MODE | command/query

Gets or sets the scramble code mode for a downlink signal.

Command Syntax: | [:SENSe]:WCDMa[:FORMat]:SCRamble:MODE <value>
<value> | ::= | "Standard" | "Left" | "Right"
Query Syntax: | [:SENSe]:WCDMa[:FORMat]:SCRamble:MODE?
Returns | ::= | "Standard" | "Left" | "Right"
Remarks: | <none>
Example: |
    :WCDM:SCR:MODE "Standard"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.ScrambleCodeMode Agilent.SA.Vsa.Wcdma.ScrambleCodeMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |