[:SENSe]:INPut:CORRection:IF:ENABle | command/query

Gets or sets a value indicating whether the calibration data in IFExternalCalibrationFile is used to correct the input data.

Command Syntax: | [:SENSe]:INPut:CORRection[1:N]:IF:ENABle <isEnabled>
<isEnabled> | ::= | 0 | 1
Query Syntax: | [:SENSe]:INPut:CORRection[1:N]:IF:ENABle?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :INP:CORR:IF:ENAB 0
Version: | 16.20 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.InputCorrection.IsIFExternalCorrectionEnabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |