[:SENSe]:W16E[:FORMat]:SUBFrame:TYPE | command/query

Gets or sets which subframe to analyze within the analysis frame.

Command Syntax: | [:SENSe]:W16E[:FORMat]:SUBFrame:TYPE <value>
<value> | ::= | "Downlink" | "Uplink"
Query Syntax: | [:SENSe]:W16E[:FORMat]:SUBFrame:TYPE?
Returns | ::= | "Downlink" | "Uplink"
Remarks: | <none>
Example: |
    :W16E:SUBF:TYPE "Downlink"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.SubframeType Agilent.SA.Vsa.Ieee80216Ofdma.SubframeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |