[:SENSe]:LTE:PROFile:ULINk:USER:PUSCh:FREQuency:HOP | command/query

Gets or sets the higher layer parameter FreqHopping used for the determination of Freq Hopping Type

Command Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUSCh:FREQuency:HOP <value>
<value> | ::= | "Off" | "InterSF00" | "IntraInterSF00" | "InterSF01" | "IntraInterSF01" | "InterSF10" | "IntraInterSF10" | "TwoInterSF" | "TwoIntraInterSF"
Query Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUSCh:FREQuency:HOP?
Returns | ::= | "Off" | "InterSF00" | "IntraInterSF00" | "InterSF01" | "IntraInterSF01" | "InterSF10" | "IntraInterSF10" | "TwoInterSF" | "TwoIntraInterSF"
Remarks: | <none>
Example: |
    :LTE:PROF:ULIN:USER:PUSC:FREQ:HOP "Off"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.Pusch.FreqHopping Agilent.SA.Vsa.Lte.FrequencyHoppingType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |