:TRACe:DEMod:FREQuency:UNIT | command/query

Gets or sets the type of X-axis unit associated with demod frequency (OFDM) data.

Command Syntax: | :TRACe[1:N]:DEMod:FREQuency:UNIT <value>
<value> | ::= | "Hertz" | "Carrier"
Query Syntax: | :TRACe[1:N]:DEMod:FREQuency:UNIT?
Returns | ::= | "Hertz" | "Carrier"
Remarks: | <none>
Example: |
    :TRAC:DEM:FREQ:UNIT "Hertz"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Trace.DemodFreqUnit Agilent.SA.Vsa.TraceFreqUnit

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |