:CALibration:ALL | command/query

Performs a full calibration of the input hardware.

Command Syntax: | :CALibration:ALL
Query Syntax: | :CALibration:ALL?
Returns | ::= | 0 | 1
Remarks: | Query form blocks until calibration is complete. Returns 1 if successful; 0 if an error occurs.
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Calibration.Calibrate

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |