[:SENSe]:LTE:CHANnel:POFFset | command/query

Set the phase offset of measurement input channel relative to the reference InputChannel in degrees.

Command Syntax: | [:SENSe]:LTE:CHANnel[1:N]:POFFset <offset>
<offset> | ::= | Real number
Query Syntax: | [:SENSe]:LTE:CHANnel[1:N]:POFFset?
Returns | ::= | Real number
Remarks: | <none>
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.SetPhaseOffsetCorrection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |