[:SENSe]:LTE:DECode:PDCCh | command/query

Gets or sets the PDCCH Bit Vector Selection to be applied.

Command Syntax: | [:SENSe]:LTE:DECode:PDCCh <value>
<value> | ::= | "Mapped" | "Demapped" | "DeInterleaved" | "Descrambled" | "DeRateMatched" | "Decoded"
Query Syntax: | [:SENSe]:LTE:DECode:PDCCh?
Returns | ::= | "Mapped" | "Demapped" | "DeInterleaved" | "Descrambled" | "DeRateMatched" | "Decoded"
Remarks: | <none>
Example: |
    :LTE:DEC:PDCC "Mapped"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PdcchBitVectorSelect Agilent.SA.Vsa.Lte.PdcchBitVectorSelectType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |