[:SENSe]:LTE:PROFile:PRS:SUBFrames | command/query

Gets or sets the number of consecutive downlink sub-frames (N_PRS) in which P-RS is transmitted.

Command Syntax: | [:SENSe]:LTE:PROFile:PRS:SUBFrames <value>
<value> | ::= | "N1" | "N2" | "N4" | "N6"
Query Syntax: | [:SENSe]:LTE:PROFile:PRS:SUBFrames?
Returns | ::= | "N1" | "N2" | "N4" | "N6"
Remarks: | <none>
Example: |
    :LTE:PROF:PRS:SUBF "N1"
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.NumberOfPositioningRsSubframes Agilent.SA.Vsa.Lte.NumberOfPositioningRsSubframesType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |