[:SENSe]:TDSCdma:ADVanced:SLOT:FREQuency:REFerence | command/query

Gets or sets what to use for the slot frequency reference.

Command Syntax: | [:SENSe]:TDSCdma:ADVanced:SLOT:FREQuency:REFerence <value>
<value> | ::= | "Pilot" | "Midamble"
Query Syntax: | [:SENSe]:TDSCdma:ADVanced:SLOT:FREQuency:REFerence?
Returns | ::= | "Pilot" | "Midamble"
Remarks: | <none>
Example: |
    :TDSC:ADV:SLOT:FREQ:REF "Pilot"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Tdscdma.Interfaces.MeasurementExtension.SlotFrequencyReference Agilent.SA.Vsa.Tdscdma.SlotFrequencyReferenceType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |