[:SENSe]:RBW:COUPle | command/query

Gets or sets how ResBW is coupled to the frequency span.

Command Syntax: | [:SENSe]:RBW:COUPle <value>
<value> | ::= | "Auto" | "Offset" | "Fixed"
Query Syntax: | [:SENSe]:RBW:COUPle?
Returns | ::= | "Auto" | "Offset" | "Fixed"
Remarks: | <none>
Example: |
    :RBW:COUP "Auto"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Frequency.ResBWCouple Agilent.SA.Vsa.ResBWCoupleType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |