[:SENSe]:EVDO:CHANnel:ACDMode | command/query

Gets or sets whether the active channel(s) are auto-detected or manually specified.

Command Syntax: | [:SENSe]:EVDO:CHANnel:ACDMode <value>
<value> | ::= | "Automatic" | "PreDefined" | "SemiAutomatic"
Query Syntax: | [:SENSe]:EVDO:CHANnel:ACDMode?
Returns | ::= | "Automatic" | "PreDefined" | "SemiAutomatic"
Remarks: | <none>
Example: |
    :EVDO:CHAN:ACDM "Automatic"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Cdma1xEvdo.Interfaces.MeasurementExtension.ActiveChannelDetectionMode Agilent.SA.Vsa.Cdma1xEvdo.ActiveChannelDetectionModeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |