[:SENSe]:LTE[:FORMat]:DLINk:PRS | command/query

Gets or sets the downlink RS PRS type (Downlink only).

Command Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:PRS <value>
<value> | ::= | "Auto" | "PN9" | "Ones" | "Custom"
Query Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:PRS?
Returns | ::= | "Auto" | "PN9" | "Ones" | "Custom"
Remarks: | <none>
Example: |
    :LTE:DLIN:PRS "Auto"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.DownlinkPilotPrs Agilent.SA.Vsa.Lte.PilotPrsType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |