[:SENSe]:WCDMa[:FORMat]:DIRection | command/query

Gets or sets the link direction for the demodulation measurement.

Command Syntax: | [:SENSe]:WCDMa[:FORMat]:DIRection <value>
<value> | ::= | "Downlink" | "Uplink"
Query Syntax: | [:SENSe]:WCDMa[:FORMat]:DIRection?
Returns | ::= | "Downlink" | "Uplink"
Remarks: | <none>
Example: |
    :WCDM:DIR "Downlink"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.Direction Agilent.SA.Vsa.Wcdma.Direction

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |