:TRACe:DEMod:EYE:LENGth | command/query

Gets or sets the digital demodulation x-axis eye length for eye diagram formats.

Command Syntax: | :TRACe[1:N]:DEMod:EYE:LENGth <value>
<value> | ::= | Real number
Query Syntax: | :TRACe[1:N]:DEMod:EYE:LENGth?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Trace.XEyeLength

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |