[:SENSe]:GSM[:FORMat]:SYNC | command/query

Gets or sets the method used to synchronize to a time slot in the measured signal.

Command Syntax: | [:SENSe]:GSM[:FORMat]:SYNC <value>
<value> | ::= | "Tsc" | "RFAmplitude" | "PolarModulationTsc" | "None"
Query Syntax: | [:SENSe]:GSM[:FORMat]:SYNC?
Returns | ::= | "Tsc" | "RFAmplitude" | "PolarModulationTsc" | "None"
Remarks: | <none>
Example: |
    :GSM:SYNC "Tsc"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.GsmEdgeEvolution.Interfaces.MeasurementExtension.SynchronizationMode Agilent.SA.Vsa.GsmEdgeEvolution.SynchronizationMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |