[:SENSe]:LTE:DECode:PUCCh | command/query

Gets or sets the PUCCH Bit Vector Selection to be applied.

Command Syntax: | [:SENSe]:LTE:DECode:PUCCh <value>
<value> | ::= | "Mapped" | "Descrambled" | "Decoded"
Query Syntax: | [:SENSe]:LTE:DECode:PUCCh?
Returns | ::= | "Mapped" | "Descrambled" | "Decoded"
Remarks: | <none>
Example: |
    :LTE:DEC:PUCC "Mapped"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PucchBitVectorSelect Agilent.SA.Vsa.Lte.PucchBitVectorSelectType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |