:INPut:DATA[:FEED] | command/query

Sets the input source to hardware or recording.

Command Syntax: | :INPut:DATA[:FEED] <feed>
<feed> | ::= | HW | REC
Query Syntax: | :INPut:DATA[:FEED]?
Returns | ::= | HW | REC
Remarks: | <none>
Example: |
    INPut:DATA REC or INP:DATA HW
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Input.DataFrom

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |