[:SENSe]:LTE:PROFile:DLINk:USER:ACTive | command/query

Gets or sets a value indicating whether the channel is present in the signal.

Command Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:ACTive <active>
<active> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:ACTive?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:PROF:DLIN:USER:ACT 0
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.DownlinkUser.Active

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |