[:SENSe]:LTE:PROFile:EPRE:ENABle | command/query

Gets or sets a value indicating whether the Per-antenna EPRE is used or the CW0/CW1 Power Boost is used to specify the power levels of users/allocations

Command Syntax: | [:SENSe]:LTE:PROFile:EPRE:ENABle <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:EPRE:ENABle?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:PROF:EPRE:ENAB 0
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.IsUsePerAntennaEpre

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |