[:SENSe]:LTE:DECode:TDD:ACKNack:MODE | command/query

Gets or sets the TDD PUSCH/PUCCH Ack/Nack Feedback Mode to be applied.

Command Syntax: | [:SENSe]:LTE:DECode:TDD:ACKNack:MODE <value>
<value> | ::= | "Bundling" | "Multiplexing"
Query Syntax: | [:SENSe]:LTE:DECode:TDD:ACKNack:MODE?
Returns | ::= | "Bundling" | "Multiplexing"
Remarks: | <none>
Example: |
    :LTE:DEC:TDD:ACKN:MODE "Bundling"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PuxchTddAckNackFeedbackMode Agilent.SA.Vsa.Lte.PuxchTddAckNackFeedbackModeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |