:TRACe:MARKer:BANDwidth:POWer:Q | query

Gets the last calculated band power result for the Q part of dual I/Q data.

Query Syntax: | :TRACe[1:N]:MARKer[1:N]:BANDwidth:POWer:Q?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Marker.BandPowerResultQ

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |