[:SENSe]:W11A:STANdard | command/query

Gets or sets the signal standard used by the transmitter.

Command Syntax: | [:SENSe]:W11A:STANdard <value>
<value> | ::= | "Ieee80211A" | "Hiperlan2" | "Ieee80211GDsssOfdm" | "Ieee80211ATurbo" | "AstmDsrc" | "Ieee80211JHalf"
Query Syntax: | [:SENSe]:W11A:STANdard?
Returns | ::= | "Ieee80211A" | "Hiperlan2" | "Ieee80211GDsssOfdm" | "Ieee80211ATurbo" | "AstmDsrc" | "Ieee80211JHalf"
Remarks: | <none>
Example: |
    :W11A:STAN "Ieee80211A"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211Agjp.Interfaces.MeasurementExtension.Standard Agilent.SA.Vsa.Wlan80211Agjp.Standard

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |