[:SENSe]:W16D[:FORMat]:STANdard | command/query

Gets or sets the signal standard used by the transmitter.

Command Syntax: | [:SENSe]:W16D[:FORMat]:STANdard <value>
<value> | ::= | "Ieee80216A" | "Ieee80216"
Query Syntax: | [:SENSe]:W16D[:FORMat]:STANdard?
Returns | ::= | "Ieee80216A" | "Ieee80216"
Remarks: | <none>
Example: |
    :W16D:STAN "Ieee80216A"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdm.Interfaces.MeasurementExtension.Standard Agilent.SA.Vsa.Ieee80216Ofdm.Standard

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |