[:SENSe]:W11B:FILTer:REFerence | command/query

Gets or sets the reference filter to use when demodulating the signal.

Command Syntax: | [:SENSe]:W11B:FILTer:REFerence <value>
<value> | ::= | "Rectangular" | "Gaussian" | "RaisedCosine"
Query Syntax: | [:SENSe]:W11B:FILTer:REFerence?
Returns | ::= | "Rectangular" | "Gaussian" | "RaisedCosine"
Remarks: | <none>
Example: |
    :W11B:FILT:REF "Rectangular"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211BG.Interfaces.MeasurementExtension.ReferenceFilter Agilent.SA.Vsa.Wlan80211BG.ReferenceFilter

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |