[:SENSe]:LTE:PROFile:POWer:ROUNd | command/query

Gets or sets a value indicating whether the auto-detected power levels are rounded to the nearest standard-defined levels (only for PDCCH-decode based auto-detection)

Command Syntax: | [:SENSe]:LTE:PROFile:POWer:ROUNd <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:POWer:ROUNd?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:PROF:POW:ROUN 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.IsPowerRoundedToStandard

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |