[:SENSe]:LTE:DECode:PCFich | command/query

Gets or sets the PCFICH Bit Vector Selection to be applied.

Command Syntax: | [:SENSe]:LTE:DECode:PCFich <value>
<value> | ::= | "Mapped" | "Descrambled" | "Decoded"
Query Syntax: | [:SENSe]:LTE:DECode:PCFich?
Returns | ::= | "Mapped" | "Descrambled" | "Decoded"
Remarks: | <none>
Example: |
    :LTE:DEC:PCF "Mapped"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PcfichBitVectorSelect Agilent.SA.Vsa.Lte.PcfichBitVectorSelectType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |