:CALibration:AUTO | command/query

Gets or sets a value indicating whether automatic calibration of the hardware is enabled.

Command Syntax: | :CALibration:AUTO <value>
<value> | ::= | 0 | 1
Query Syntax: | :CALibration:AUTO?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :CAL:AUTO 0
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Calibration.IsAutoCalibrateEnabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |