[:SENSe]:W11N[:FORMat]:GUARd[:INTerval]:SELection | command/query

Gets or sets how the guard interval (cyclic prefix) is determined.

Command Syntax: | [:SENSe]:W11N[:FORMat]:GUARd[:INTerval]:SELection <value>
<value> | ::= | "Invalid" | "Manual" | "Sig" | "HTSig"
Query Syntax: | [:SENSe]:W11N[:FORMat]:GUARd[:INTerval]:SELection?
Returns | ::= | "Invalid" | "Manual" | "Sig" | "HTSig"
Remarks: | <none>
Example: |
    :W11N:GUAR:SEL "Invalid"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211N.Interfaces.MeasurementExtension.GuardIntervalSelection Agilent.SA.Vsa.Wlan80211N.GuardIntervalSelection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |