[:SENSe]:LTE:ADVanced:ULINk:FREQuency:CENter | command/query

Gets or sets the center frequency of the UL signal, to be used to determine the limits for UL spectrum flatness test.

Command Syntax: | [:SENSe]:LTE:ADVanced:ULINk:FREQuency:CENter <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:LTE:ADVanced:ULINk:FREQuency:CENter?
Returns | ::= | Real number
Remarks: | <none>
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.FrequencyCenterUL

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |