:SYSTem:VSA:HARDware:CONFiguration:ANALyzer:ROSCillator:EXTernal:FREQuency | command/query

Gets or sets the frequency of the external reference signal

Command Syntax: | :SYSTem:VSA:HARDware:CONFiguration:ANALyzer:ROSCillator:EXTernal:FREQuency <frequencyHz>
<frequencyHz> | ::= | Real number
Query Syntax: | :SYSTem:VSA:HARDware:CONFiguration:ANALyzer:ROSCillator:EXTernal:FREQuency?
Returns | ::= | Real number
Remarks: | <none>
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.HardwareConfiguration.ExternalReferenceFrequency

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |