:INPut:RECording:LENGth:MAXimum:TIME | query

Gets the maximum recording time supported by the current measurement's input channels.

Query Syntax: | :INPut:RECording:LENGth:MAXimum:TIME?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Recording.RecordLengthMaximumTime

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |