[:SENSe]:W11B:ADVanced:DESCramble | command/query

Gets or sets which parts of the signal to descramble.

Command Syntax: | [:SENSe]:W11B:ADVanced:DESCramble <value>
<value> | ::= | "On" | "Off" | "Preamble" | "PreambleHeader"
Query Syntax: | [:SENSe]:W11B:ADVanced:DESCramble?
Returns | ::= | "On" | "Off" | "Preamble" | "PreambleHeader"
Remarks: | <none>
Example: |
    :W11B:ADV:DESC "On"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211BG.Interfaces.MeasurementExtension.DescrambleMode Agilent.SA.Vsa.Wlan80211BG.DescrambleMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |