[:SENSe]:WCDMa:CHANnel:DESPread:DLINk:MOD | command/query

Gets or sets the modulation for the despread channel in downlink measurements.

Command Syntax: | [:SENSe]:WCDMa:CHANnel:DESPread:DLINk:MOD <value>
<value> | ::= | "Qpsk" | "Qam16" | "Qam64"
Query Syntax: | [:SENSe]:WCDMa:CHANnel:DESPread:DLINk:MOD?
Returns | ::= | "Qpsk" | "Qam16" | "Qam64"
Remarks: | <none>
Example: |
    :WCDM:CHAN:DESP:DLIN:MOD "Qpsk"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.DownlinkChannelModulation Agilent.SA.Vsa.Wcdma.DownlinkChannelModulation

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |