:TRACe:DEMod:TIME:UNIT | command/query

Gets or sets the type of X-axis unit associated with demodulation time data.

Command Syntax: | :TRACe[1:N]:DEMod:TIME:UNIT <value>
<value> | ::= | "Second" | "Symbol"
Query Syntax: | :TRACe[1:N]:DEMod:TIME:UNIT?
Returns | ::= | "Second" | "Symbol"
Remarks: | <none>
Example: |
    :TRAC:DEM:TIME:UNIT "Second"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Trace.DemodTimeUnit Agilent.SA.Vsa.TraceTimeUnit

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |