:TRACe:SPECtrogram:THReshold | command/query

Gets or sets the threshold, which affects the minimum amplitude value that will be shown in the spectrogram / 3D map.

Command Syntax: | :TRACe[1:N]:SPECtrogram:THReshold <newValue>
<newValue> | ::= | Real number
Query Syntax: | :TRACe[1:N]:SPECtrogram:THReshold?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Spectrogram.Threshold

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |