:INPut:ANALog:MIXer:LEVel:LIST | command/query

Gets or sets the mixer level in dB relative to the factory default setting for the input channel.

Command Syntax: | :INPut:ANALog:MIXer:LEVel:LIST <mixerLevel>
<mixerLevel> | ::= | Comma separated values of Real number
Query Syntax: | :INPut:ANALog:MIXer:LEVel:LIST?
Returns | ::= | Comma separated values of Real number
Remarks: | <none>
Example: |
    :INP:ANAL:MIX:LEV:LIST 0.0,0.0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.AnalogChannel.MixerLevel

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |