[:SENSe]:LTE:PROFile:RB:AUTO:MODE | command/query

Gets or sets a value indicating whether RB Auto Detection is power-based or PDCCH-decode-based

Command Syntax: | [:SENSe]:LTE:PROFile:RB:AUTO:MODE <value>
<value> | ::= | "PowerBased" | "DecodeBased"
Query Syntax: | [:SENSe]:LTE:PROFile:RB:AUTO:MODE?
Returns | ::= | "PowerBased" | "DecodeBased"
Remarks: | <none>
Example: |
    :LTE:PROF:RB:AUTO:MODE "PowerBased"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.RBAutoDetectMode Agilent.SA.Vsa.Lte.RBAutoDetectModeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |