:INPut:TRIGger:FMASk:CRITeria | command/query

Gets or sets the criteria for when a trigger will occur for a given signal relative to the mask.

Command Syntax: | :INPut:TRIGger:FMASk:CRITeria <value>
<value> | ::= | "Enter" | "Leave" | "Inside" | "Outside" | "EnterThenLeave" | "LeaveThenEnter"
Query Syntax: | :INPut:TRIGger:FMASk:CRITeria?
Returns | ::= | "Enter" | "Leave" | "Inside" | "Outside" | "EnterThenLeave" | "LeaveThenEnter"
Remarks: | <none>
Example: |
    :INP:TRIG:FMAS:CRIT "Enter"
Version: | 17.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.FrequencyMaskTrigger.Criteria Agilent.SA.Vsa.FrequencyMaskTriggerCriteria

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |